Search Tips

Search is based on keyword.

`Ex: "Procedures"`

Do not search with natural language

`Ex: "How do I write a new procedure?"`

Give Feedback Support Portal

# Monitor Output in Hiero (SDI/HDMI)

The Monitor Out feature allows you to preview a timeline Viewer image in a floating window, NDI session, or on an external projector/video monitor to check the final result, including the correct output transform and aspect ratio.

A dedicated Viewer Monitor Out workspace provides easy access to the monitor out strip and its controls in the Properties panel.

Hiero supports internal monitor out using a Floating Window, NDI sessions, and dedicated AJA or Blackmagic cards, selected from the Device dropdown in the ViewerMonitorOut's Properties:

• Floating Window - Hiero's native monitor out uses a floating monitor and does not require additional hardware. Mac users can also take advantage of additional HDR technology including an extended sRGBf LUT. See Working with HDR Images for more information.

• NDI - A network protocol that enables video and metadata signals to be sent over standard IP networks in real-time. This option allows you to easily share a stream of the Viewer output to anyone else on the same network.

Note: To view the NDI stream, you need the NDI Studio Monitor or NDI Video Monitor application installed. See Streaming Viewer Output Over the Internet with NDI® for more information.

• Dedicated AJA or Blackmagic Design cards - Hiero supports various AJA and Blackmagic devices that can be selected from the Device dropdown after installation. See AJA and Blackmagic Design Monitor Out Devices for more information on supported hardware and drivers.

Note: Audio scrubbing is not currently available through monitor out cards. Audio scrubbing is only supported through internal audio output devices.

# Enabling Hiero Monitor Out

Hiero's monitor out uses a floating monitor, NDI session, or additional hardware from AJA or Blackmagic to display monitor out. The floating monitor allows Mac users to take advantage of additional HDR technology including an extended sRGBf LUT. See Working with HDR Images for more information.

| 1. | Navigate to Workspace > Viewer Monitor Out.

The Viewer Monitor Out workspace is displayed with the Monitor Out toolbar under the Viewer by default.

If you're working with multi-view footage in Interactive buffer mode, the monitor shows the output from the selected Viewer including the A/B player mode currently in use, such as wipe or difference. In Active, Buffer A, or Buffer B mode, additional controls display to determine the stereo mode and view to output. See Stereoscopic and Multi-View Projects for more information.

| 2. | Click the cog icon in the Viewer Monitor Out panel to display the Properties panel.

| 3. | Select the device you want to use from the output Device dropdown. All available devices are automatically detected and listed in this menu, along with the default options:

• Floating Window - opens a floating monitor window, without the need for a monitor device and card. This is intended for full-screen use without displaying any of the interface.

Tip: Disable Minimize with Application to allow the floating window to remain visible when Hiero is minimized.

• NDI - A network protocol that enables video and metadata signals to be sent over standard IP networks in real-time. This option allows you to easily share a stream of the Viewer output to anyone else on the network.

Note: To view the NDI stream, you need the NDI Studio Monitor or NDI Video Monitor application installed. See Streaming Viewer Output Over the Internet with NDI® for more information.

• Installed Cards - transfers the Viewer contents to the selected card and displays SDK and driver information associated with the card.

The Viewer Monitor Out and Properties panel duplicate some controls for convenience.

| Viewer | Select the Viewer to feed to the output monitor using the source viewer dropdown. Selecting Active Viewer always displays the Viewer that is currently selected in the workspace. In this dropdown, you also have the option to select a Contact Sheet to display. They're interchangeable as long as you're in Interactive mode (see item 2 below).
|  | Select the view mode using the AB Mode dropdown: • Active Buffer - the monitor always shows the output from the buffer currently in use by the selected Viewer. • Buffer A - the monitor always shows the output from the selected Viewer buffer A. • Buffer B - the monitor always shows the output from the selected Viewer buffer B. • Interactive - the monitor shows the output from the selected Viewer including the A/B player mode currently in use, such as wipe or difference. Note: Interactive mode's GUI-Independent Resolution ensures that workspace layout does not compromise image fidelity, ensuring correct framing, independent color transforms, and synchronized zooming and panning.
| Display Mode | Select the resolution output from the monitor card currently in use. The resolutions available depend on the card manufacturer. Note: Floating monitor out always uses the resolution of the Viewer in use.
| Pixel Format | Select the pixel format output from the monitor card currently in use. The formats available depend on the card manufacturer.
|  | Click the button or enable Use Viewer Gamma, Gain and Saturation to apply the active Viewer’s filtering, gamma, gain and saturation to the monitor out.
|  | Click the button or enable Vertical Flip to flip the output vertically. This control is handy if you're using a ceiling mounted projector.
|  | Click the button or enable Horizontal Flip to flop the output horizontally.
|  | Click to enable the mouse pointer position on the monitor. You can control the size of the cursor on the monitor in the Preferences under Panels > Viewer (Monitor Out) > Mouse Pointer Scale.
|  | Click to display annotations active in the selected timeline Viewer on the monitor for review purposes. See Annotations for more information. Note: This option is not supported when viewing Contact Sheet.
| Output Transform | Select the color transform to apply to the image. If you’ve specified an OCIO configuration file in the preferences, these custom LUTs are also applicable.

Note: When viewing a Contact Sheet, an additional option, HUD Text Scale, is available in this panel, allowing you to change the text scale of the HUD metadata overlay, which only affects Contact Sheet in Monitor Out.

# AJA and Blackmagic Design Monitor Out Devices

Our monitor out architecture interfaces directly with the AJA and BlackMagic Design device drivers, which are unified across their respective hardware lines, meaning all current supported cards for the versions detailed in Third-Party Libraries and Fonts should work.

You can select installed cards from the MonitorOut's Properties panel using the Device control. The SDK and driver versions for the selected card are displayed for convenience.

We've tested the following AJA and Blackmagic Design hardware:

AJA Card: | KONA 4 | KONA 5 | KONA iO4k+ | T-Tap Pro
--- | --- | --- | --- | ---
See https://www.aja.com/family/desktop-io and https://www.aja.com/products/t-tap-pro#techspecs for more details on supported formats.
Connection |
BNC |  |  |  |
HDMI |  |  |  |
Stereoscopic Support |
| Yes | Yes | No | No
Platforms |
| Win, Mac, Linux | Win, Mac, Linux | Win, Mac, Linux | Win, Mac
Drivers |
| Driver 16.2.5 or later, available here: • Windows: https://www.aja.com/assets/support/files/9149/en/AJA-Software-Installer_Windows_v16.2.5_Release.zip • macOS: https://www.aja.com/assets/support/files/9146/en/AJA-Software-Installer_macOS_v16.2.5_Release.zip • Linux: https://www.aja.com/assets/support/files/9140/en/AJA-Software-Installer_Linux_RedHat_CentOS_v16.2.5_Release.zip |

Blackmagic Card: | UltraStudio 4K Mini | 4K Extreme | 4K Extreme 12G | 8K Pro
--- | --- | --- | --- | ---
See https://www.blackmagicdesign.com/uk/products/ for more details on supported formats per card.
Connection
BNC |  |  |  |
HDMI |  |  |  |
Stereoscopic Support
| No | No | Yes | No
Platforms
| Win, Mac, Linux | Win, Mac, Linux | Win, Mac, Linux | Win, Mac, Linux
Drivers
| Driver 12.4.2.0 or later, available here: • Windows: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Windows • macOS: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Mac%20OS%20X • Linux: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Linux

Blackmagic Card: | DeckLink Studio 4K | DeckLink 4K Extreme | DeckLink 4K Extreme 12G
--- | --- | --- | ---
See https://www.blackmagicdesign.com/uk/products/ for more details on supported formats per card.
Interface
BNC |  |  |
HDMI |  |  |
Stereoscopic Support
| Yes (Both views through one output, so the Full Resolution option is not available.) | Yes | Yes
Platforms
| Win, Mac, Linux | Win, Mac, Linux | Win, Mac, Linux
Drivers
| Driver 12.4.2.0 or later, available here: • Windows: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Windows • macOS: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Mac%20OS%20X • Linux: https://www.blackmagicdesign.com/support/download/2438c76b9f734f69b4a914505e50a5ab/Linux

Some monitor out cards allow you to extend or mirror your desktop so that the user interface is visible on the monitor. Please refer to your card’s documentation for more information.